Psuedo Rapidity

UA5 Minimum bias data and non single diffractive data

UA5 minimum bias data (dots) is compared with Adhoc Model (lines) at root s, 900, 546, 200 and 53 GeV

We must be careful when we compare the data with simulation. Non single diffractive data (+) gives higher yield than minimum bias data(square). The Monte Carlo simulation must be compared with the minimum bias inelastic data.